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Clipping Points – Yard Operation
SOP-006

1: Introduction
Point clips are used to secure points in the normal or reverse position.  

Facing points on running lines must be locked if:  

· you cannot be sure that the points will remain in the correct position, or 
· there is an instruction at the points to clip and lock them.

A lock may also be used on the clip to ensure the point clip is not removed, authority to use a lock or not is with the Track Manager. 

2: Using Point Clips
Use standard point clips for standard points. Standard points have a switch blade and stock rail of similar depth. The standard point clip has a simple hook for the switch blade flange. 
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